How to load OS on to HC3.

1. Load information from file on to microSD card. Do not place in any folders. Load direct to root.
2. Take out the battery and put microSD card in unit.
3. Reinsert the battery but leave off battery door
4. Press and hold the home and power keys at the same time unit red text stating that the new OS is loading appears on the “Performance Power Accuracy” Screen.
5. Once it has completed loading, the HC3 will reboot and the new OS will be on the HC3.
6. Perform the screen calibration by following the instructions that appear.
7. Set unit to desired date, time, and time zone.